0x05EC Skip Steps

Use this TLV in the Play File Modify message when the Action field is set to Skip Forward or Skip Backward.

Byte | Description
0, 1 | Tag 0x05EC Skip Steps
2, 3 | Length 0x0002
4, 5 | Value[0-1] Steps (100 ms increments) Minimum 1 (0x0001) Maximum 65534 (0xFFFE) Start of File 0 (0x0000) End of File 65535 (0xFFFF)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.