0x09CD Delete Global Title Entry

After the deleted Global Title (GT) Entry TLV is executed, the deleted GT Entry is not out of service immediately. It is used to do GTT until the index table is built which remove these GT entries from the GT table.

Used in:
SS7 SCCP TCAP Configure message

Byte | Description
0, 1 | Tag 0x09CD Delete Global Title Entry
2, 3 | Length Variable
4 | Value[0] Group ID 1-127 Already configured.
5 | Value [1] Entry Attribute (ATT) Bit 0 - Wild Card bit 0 = Non-Wild Card GT 1 = Wild Card GT Bits 1-7 Not Used.
6 | Reserved for future use.
7 | Value [2] Global Title Address Information Length 1-24 digits
: | Value [n] Global Title Address Information (GTAI) See Table 4-1 for format.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Signaling System Number Seven.
See Transaction Capability Application Part.