0x0607 Output Gain Control

Use this TLV to set the output gain, in decibels, for a conference.

It is used in the in the following messages

Generic Card Configure (0x0122)
R esource Create (0x0124)

Resource Modify (0x0125)

Resource Connect (0x0127) .

Byte | Description
0, 1 | Tag: 0x0607 - Output Gain Control
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Output Gain (1 db steps) Minimum: -40 (0xFFD8) Maximum: 0 (0x0000) Default: 0 (0x000A)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.