You are here: SwitchKit® Development Environment Programmer’s Guide > 9 Addressing Functions > AIB Manipulation Functions

AIB Manipulation Functions

Description

These functions are designed to provide assistance to the application developer in initializing the information contained in various AIBs as described in the API Reference.

How Applications use AIB Functions

You must use the appropriate functions for initializing the AIBs. Using the wrong functions or not using all the functions necessary to completely initialize an AIB may result in an improperly defined AIB. See AIB Manipulation Functions and SS7 Addressing Functions for a mapping of the functions and AIBs. When attempting to initialize a Range of Channels (0x0D) AIB, you must call all of the following functions:

• setAIBStartSpan()

• setAIBStartChannel()

• setAIBEndSpan()

• setAIBEndChannel()

See Address Information Block.