You are here: SwitchKit® Development Environment - CSA User’s Guide > 2 Basic Configuration - System/Node > Reading a Configuration from SwitchManager

Reading a Configuration from SwitchManager

This procedure describes how to read an existing configuration from SwitchManager.

Before you begin

The LLC and SwitchManager must be running and a configuration must be applied to your CSP. The CSA must be started.

Read Configuration

The following steps explain how to read the configuration from SwitchManager.

1 Go to the File menu, select Read Configuration from SwitchManager. If you are not already connected to the LLC, this opens the Connect to LLC dialog.

2 Specify the Label. This may be alphanumeric and must contain no spaces.

3 Fill in the other fields, if necessary. This depends on your system setup.

4 Click OK to close the Connect to LLC dialog box.

See Converged Services Administrator.