0x05E6 File Event Descriptor

Use this TLV in the Play File Start Record File Start messages to configure the generation of Call Processing Events related to the playing and recording of files..

Byte | Description
0, 1 | Tag: 0x05E6 File Event Descriptor
2, 3 | Length: 0x0001
4 | Value[0]: File Event Descriptor Mask Default = 0x00 Bit 0 If set, Call Processing Event of "Play File Completed" (0x2C) is generated when the file finishes playing. Bit 1 If set, Call Processing Event of "Play File Started" (0x2B) is generated when the file begins playing. Bit 2 If set, Call Processing Event of "Record File Completed" (0x2E) is generated when the file finishes recording. Bit 3 If set, Call Processing Event of "Record File Started" (0x2D) is generated when the file begins recording. Bits 4-7 Reserved (must be 0x00)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.