You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Card Views in Monitoring Mode

Card Views in Monitoring Mode

The CSA offers different card views for the different card types in your system.

Open Card Views

Double-click the card you want to view in the node view window to open a card view. See the next screen shot of a node view in monitoring mode.

Card Properties

The Card Properties... window contains information about the slot where the selected card is located. To get to a card’s properties, right-click the slot of a card in the node view in monitoring mode, and then select Card Properties from the pop-up menu. You will see information such as, the Serial Number, PC Art Work Revision, Functional Revision, ROM Revision, RAM Revision, and RAM Build. The properties’ windows are view-only. You cannot change any settings. As an example, the card properties for the IP Network Series 2 card are shown in the screen shot. This card also shows the Motherboard DIP Switch Settings.

See Converged Services Administrator.
Read Only Memory
Random Access Memory
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.