0x05ED Dual Channel Record Option

Use this TLV when recording a conference with the Record File Start message to choose whether you want each channel to be saved to its own file or both channels to be saved to the same file.

Byte | Description
0, 1 | Tag 0x05ED Dual Channel Record Option
2, 3 | Length 0x0001
4 | Value[0] 0x00 Sum Channels Together (Default) 0x01 Independent Channels (file location is the same, but filename is appended with "_ 2" )

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.