0x04 Server Socket Register by Name

Used in:
IP Socket Configure message

Byte | Description
0 | Tag 0x04 Server Socket Register by Name
1 | Length Variable
2 | Value[0] 0x00 Module (0xFF = Main Board)
3 | Value[1] Socket ID
4-7 | Value[2-5] Local IP Address (4 bytes)
8, 9 | Value[6, 7] Local Port
10 | Value[8] Remote Name Length
11 | Value[9] Remote Name[0]
12 | Value[10] Remote Name[1]
13 | Value[:]
: | Value[:] Remote Port
: | Value[:] Remote Port

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."