You are here: CSP Developer’s Guide: Overview > 6 Layer 4 Call Control PPL Information > PC - Physical Connection Management (0x0063)

PC - Physical Connection Management (0x0063)

PPL Events

The table below shows the PPL Events sent to PC from the CM component.

Event | Description
--- | ---
(1) L4PCevL4CM_LOCAL_CALL_CONNECT_REQUEST | Request to connect voice path from the local channel
(2) L4PCevL4CM_REMOTE_CALL_CONNECT_REQUEST | Request to connect voice path from the remote channel
(3) L4PCevL4CM_DISCONNECT_REQUEST | Request to disconnect voice path from the remote channel
(4) L4PCevL4CM_LOCAL_CALL_FORCED_CONNECT_REQUEST | Request to immediately force connect the voice path

See Programmable Protocol Language.