0x10 Cadence Ringing Extended
(Type C - Digits Missing, Characters Present)

Data[0] Type 0x10
Data[1] Length
Data[2] Cadence Ringing Type
Data[3] Month (binary)
Data[4] Day (binary)

Data[5] Hour (binary)

Data[6] Minute (binary)
Data[7] CLIP RAI Parameter Type 0x04
Data[8] CNIP CNI Parameter Type 0x07
Data[9] Reason for Absence of Digits

Data[10] Number of Characters in Calling Party

Data[11] Calling Party Digit 2 (ASCII)
Character 1
Character 2
Character M

Pattern of tones and silence, such as a busy signal.
American Standard Code for Information Interchange