0x0006 Add V5 User Port Range

Used in:
V5 Configure message
V5 Configuration Query message

Byte | Description
0 | Tag 0x00 Add V5.2 User Port Range (MSB)
1 | Tag 0x06 Add V5.2 User Port Range (LSB)
2 | Length 0x00 (MSB)
3 | Length 0xNN (LSB)
4 | Number of Ranges
5 | User Port Type
6 | Start User Port ID, MSB
7 | Start User Port ID, LSB
8 | End User Port ID, MSB
9 | End User Port ID, LSB
: | :
: | Start User Port ID, MSB
: | Start User Port ID, LSB
: | End User Port ID, MSB
: | End User Port ID, LSB
: | :

The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Most Significant Bit
Least Significant Bit