0x05F5 Fixed Memory Statistics

This TLV is reported in the response to the Statistics Query message. It includes the total, average, and maximum blocks of fixed memory used on a specific DSP chip. A history of these statistics is not maintained.

Byte | Description
0, 1 | Tag: 0x05F5 - Fixed Memory Statistics
2, 3 | Length: 0x0008
4 | Value[0] Module Number 0x00 - DSP Module 0 0x01 - DSP Module 1 0xFF - Mainboard
5 | Value[1] Processor Number 0x00 - 0x03 0x00 for processor on Main board
6, 7 | Value[2, 3] Total Blocks
8, 9 | Value[4, 5] Average Blocks Used
10, 11 | Value[6, 7] Max Blocks Used

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor