0x060A Echo Suppression Enable

Use this TLV to enable and disable echo suppression in a conference.

It is used in the following messages

Generic Card Configure (0x0122)

R esource Create (0x0124)

Resource Modify (0x0125)

Resource Connect (0x0127)

Byte | Description
0, 1 | Tag: 0x060A Echo Suppression Enable
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Echo Suppression 0x0000 - Disabled (Default) 0x0001 - Enable

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.