0x05EB Maximum Record Timer

Use this TLV in the Record File Start message to set the maximum length of time allowed for recording a message.

Byte | Description
0, 1 | Tag 0x05EB Maximum Record Timer
2, 3 | Length 0x0002
4, 5 | Value[0-1] Timer (10 ms increments) Minimum 1 (0x0001) Maximum 65534 (0xFFFE) Disable timer 65535 (0xFFFF) (Default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.