0x05F9 Query Statistics

Use this TLV in the Statistics Query message to indicate the Query Type and Sample Number.

Byte | Description
0, 1 | Tag: 0x05F9 - Query Statistics
2, 3 | Length: 0x0004
4, 5 | Value[0, 1] Query Type 0x0400 - DSP Function Statistics 0x0401 - NFS Statistics 0x0402 - Fixed Memory Statistics 0x0403 - DSP Series 2 Cache Statistics 0x0404 - Resource Point Statistics 0x0405 - CPU Statistics 0x0406 - DSP 2 Overload Statistics 0xFFFF - Returns all valid Queries for the entity queried.
6, 7 | Value[2-3]: Sample Number 0x0000 - Current Working Buffer 0x0001- 0x0010 - Saved copies [N-1], N-2] . . . 0xFFFE - Instantaneous values of used and free channels 0xFFFF - A copy that is cleared every time it is read

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor