You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Refreshing a Configuration from SwitchManager

Refreshing a Configuration from SwitchManager

This procedure describes how to refresh an existing configuration from SwitchManager.

Before you begin

The LLC and SwitchManager must be running and a configuration must be applied to your CSP. Open the CSA.

Refresh Configuration

Do the following to refresh the configuration from SwitchManager.

1 Go to the monitoring mode of your configured node.

2 Go to the File menu, select Refresh Configuration from SwitchManager. CSA will close the current configuration file and re-read the configuration file from switchmgr to reflect any changes from dynamic configuration files.

CSA will close the current configuration file and read a fresh configuration file from SwitchManager.

See Converged Services Administrator.