You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > 5 SwitchKit TCAP Abstraction Layer > sktal_clearTCAPDialogHandler()

sktal_clearTCAPDialogHandler()

Description

The user must remove the transaction handler once the transaction has been completed (by receiving TC-U-ABORT, TC-P-ABORT, TC-END, or TC-UNI, or sending TC-U-ABORT, TC-END, or TC-UNI). It is imperative to NOT take this step until the last message for a transaction has been sent or received.

Syntax

int sktal_clearTCAPDialogueHandler(int instanceId,

unsigned dialogueId);

Input Parameters

Argument | Description
--- | ---
instanceID | Instance for given node/stack/SNN combination
dialogueId | TCAP dialogue ID

Input/Output Parameters and Output Parameters

None.

Return Value

SKTAL_SUCCESS: If method is successful.

SKTAL return code as defined in Appendix C, SKTAL Return Codes.

See Transaction Capability Application Part.