0x0679 Echo Cancel CNG Noise Threshold

Use this TLV in the Generic Card Configure message to set card-level parameters for Echo Cancel.

Byte | Description
0, 1 | Tag: 0x0679
2, 3 | Length: 0x0002
4 | Value [0] CNG Noise Threshold Maximum near end noise level used to compute CNG level 0 to 32767 Formula: 32767*10^(dBm-3)/20) dB = value you enter

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.