You are here: CSP Hardware Installation and Maintenance > A Industry Compliance > European Compliance Summary

European Compliance Summary

CE Mark Certification

Refer to European Declarations of Conformity for the specific chassis and cards that have passed the CE Mark Certification process.

R & TTE Directive

Emissions

EN55022:1998/A1:2000/A2:2003

EN55024:1998/A1:2001/A2:2003

EN 300386:2001 Rev 1.3.3

Emissions tests were performed with shielded I/O cables.

Safety

EN60950-1, CB Scheme IEC 60950-1

This equipment has been tested for applications where the Dialogic product is behind the CSU.

Telecommunications

CTR 12 Compliant, TBR12, TBR13

E-ONE 120 Ohm LC, E-ONE 120 Ohm I/O, E-ONE 120 Ohm Redundant I/O, E-ONE 120 Ohm Standby I/O

CTR 4 Compliant, TBR4

ISDN PRI package includes the E-ONE 120 Ohm interfaces.

NTR 11 Compliant

DPNSS/DASS2 package includes the E-ONE 75 Ohm interfaces.

NTR 4 Compliant

E-ONE 75 Ohm LC, E-ONE 75 Ohm I/O, E-ONE 75 Ohm Redundant I/O, E-ONE 75 Ohm Standby I/O

See Integrated Services Digital Network.