0x36 Query Host Connections

Used in:
Multi-Host Configure message

ICB Type | 0x01 (Action)
ICB ID | 0x36
Data Length | Variable
Data[0–3] | Default Host ID (4 bytes) (00 00 00 00 if not connected)
Data[4-5] | Number of hosts connected (2 bytes)
Data[6-9] | Host ID 1 (4 bytes. First connected additional host)
Data[10-13] | Host ID 2 (4 bytes)
: | :
Data[:] | Host ID N (4 bytes)

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Information Control Block.