You are here: CSP Hardware Installation and Maintenance > 3 CSP Chassis Installation > Rack Mounting

Rack Mounting

CSP 2090 and CSP 2110

You can either front-mount or mid-mount both the CSP 2090 and
CSP 2110 (CSP 2090 and CSP 2110 Mounting Bracket Options ). You can mount both in either a 48.2 cm (19-inch) rack or a 58.4 cm (23-inch) rack. The mounting brackets are reversible to accommodate either size. Use standard 10/32 mounting hardware to fasten the brackets to the sides of the chassis. (Mounting on 19-Inch and 23-Inch Racks )

Mounting Guidelines

When mounting the chassis, follow these guidelines:

Mount the chassis with another person helping you. The average weight of both the CSP 2090 and CSP 2110 base units is approximately 34 kg (75 lb).

Do not obstruct the vents of the front or rear fan tray.

Allow sufficient room to slide the fan trays out. The depth of each tray, including handles, is specified below.

Table 3-1 Fan Tray Depths

Fan Tray | CSP 2090 | CSP 2110
--- | --- | ---
Front | 31.7 cm (12.5") | 31.7 cm (12.5")
Rear | 21.0 cm (8.25") | 21.0 cm (8.25")

Avoid touching integrated circuit areas as static charges can damage circuits.

Mounting Bracket Diagram

The following illustration shows the possible locations of the mounting brackets on a CSP 2090 and CSP 2110 (CSP 2090 and CSP 2110 Mounting Bracket Options ).

Figure 3-1 CSP 2090 and CSP 2110 Mounting Bracket Options

Mounting Dimensions

Mounting on 19-Inch and 23-Inch Racks provides CSP 2090 chassis mounting information.

Figure 3-2 Mounting on 19-Inch and 23-Inch Racks

Mounting on 19-Inch Racks , Mounting on 23-Inch Racks , and Mid-Mounting on 19-Inch Rack illustrate CSP 2110 chassis mounting information.

Figure 3-3 Mounting on 19-Inch Racks

Figure 3-4 Mounting on 23-Inch Racks

Figure 3-5 Mid-Mounting on 19-Inch Rack

CSP 2040

The CSP 2040 is a front-mount chassis. You can mount the CSP 2040 in either a 19-inch rack (Dimensions for 19-Inch Rack ) or a 23-inch rack (Dimensions for 23-Inch Rack ). The CSP 2040 mounting brackets are reversible to accommodate either size. Use standard 10/32 mounting hardware to fasten the brackets to the sides of the chassis.

Mounting Guidelines

When mounting the chassis, follow these guidelines:

Mount the chassis with another person helping you. The average weight of the CSP 2040 Chassis is approximately 40 pounds.

Do not obstruct the vents of the front fan tray.

Allow sufficient room to slide the fan tray out.

Avoid touching integrated circuit areas as static charge can damage circuits.

19 Inch Mounting Option

Below is a diagram illustrating the dimensions of a CSP 2040 Chassis set to the 19-inch mounting option.

Figure 3-6 Dimensions for 19-Inch Rack

23 Inch Mounting Option

Below is a diagram illustrating the dimensions of a CSP 2040 Chassis set to the 23-inch mounting option.

Figure 3-7 Dimensions for 23-Inch Rack