You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > B Appendix - SKIM Data Types and Codes > SKIM Data Types and Codes

SKIM Data Types and Codes

Purpose

This section provides information on SKIM data types and error codes.

Table B-1

Data Types | System Data Type
--- | ---
SKIM_BOOLEAN | unsigned int.
SKIM_OCTET | unsigned char.
SKIM_USHORT | unsigned short.
SKIM_UINT | unsigned int.
SKIM_ULONG | unsigned long.
SKIM_CHAR | char
SKIM_SHORT | short
SKIM_INT | int
SKIM_LONG | long

SKIM Data Types

Table B-2 SKIM Return Codes

Error Codes | Values
--- | ---
SKIM_SUCCESS | 0
SKIM_FALSE | 0
SKIM_TRUE | 0x1
SKIM_ENOMEM | -1
SKIM_ERCVFAIL | -6
SKIM_ENOMSG | -8
SKIM_ESENDFAIL | -9
SKIM_ETCAPMSGSENDFAIL | -13
SKIM_BADTCAPMESSAGE | -16
SKIM_ETOOMANYDIALOGS | -18
SKIM_ENOINVID | -20
SKIM_ENOMUTEX | -24
SKIM_EBADMUTEX | -25
SKIM_EINVALIDARGS | -39
SKIM_ENOLICENSE | -45
SKIM_EPROTERR | -46
SKIM_EOVERFLOW | -49
SKIM_EINITFAIL | -52
SKIM_EINUSE | -55
SKIM_EDESTPROHIBIT | -56
SKIM_EINVPTYPE | -57
SKIM_EINVOPFAM | -58
SKIM_EINVOPSPEC | -59
SKIM_EINVLEN | -60
SKIM_ENULLPTR | -61
SKIM_EBADSTATE | -64
SKIM_ENOTFOUND | -65
SKIM_EASNENCODE | -66
SKIM_EASNDECODE | -67
SKIM_EINVOPC | -72
SKIM_EINVDPC | -73
SKIM_EINVINITSTATE | -86

A sequence of eight bits.