0x05FB Silence Threshold

Use this TLV in the Record File Start to set the Silence Threshold. When the Beep Amplitude is reached, silence is no longer assumed.

Byte | Description
0, 1 | Tag: 0x05FB - Silence Threshold
2, 3 | Length: 0x0001
4 | Value[0] Beep Amplitude, in decibel milliwatts (dBM) Minimum: -54 (0xCA) Maximum: 3 (0x03) Default: -25 (0xE7)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.