You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > 5 SwitchKit TCAP Abstraction Layer > sktal_sendTCAPDialog()

sktal_sendTCAPDialog()

Description

This method sends a TCAP dialogue message.

Syntax

int sktal_sendTCAPDialog(int instanceId, unsigned dialogueId, SKTAL_DLG *dlg);

Input Parameters

Argument | Description
--- | ---
instanceID | Instance for given node/stack/SNN combination
dialogueId | TCAP dialogue ID
dlg | Pointer to the structure containing TCAP dialogue information

For definition See Appendix D, SKTAL_DLG and SKTAL_CPT Structure Definitions

Input/Output Parameters and Output Parameters

None.

Return Value

SKTAL_SUCCESS: If method is successful.

SKTAL return code as defined in Appendix C, SKTAL Return Codes.

See Transaction Capability Application Part.