You are here: SwitchKit® Development Environment Programmer’s Guide > 4 Register Functions > sk_pplTCAPRegister() / sk_pplTCAPUnRegister()

sk_pplTCAPRegister() / sk_pplTCAPUnRegister()

Description

Use the function sk_pplTCAPRegister() to enable an application to register for TCAP traffic by Sub-System Number (SSN) or Origination Point Code(OPC). This message is also available as sk_pplTCAPRegisterOnConnection() and skts_pplTCAPRegister().

Use sk_pplTCAPUnRegister() to unregister. This message is also available as sk_pplTCAPUnRegisterOnConnection() and skts_pplTCAPUnRegister().

Syntax

int sk_pplTCAPRegister(int aRegisterVal, UBYTE aRegisterType);

int sk_pplTCAPUnRegister(int aRegisterVal, UBYTE aRegisterType);

int sk_pplTCAPRegisterOnConnection(int aRegisterVal, UBYTE aRegisterType, int aConID);

int sk_pplTCAPUnRegisterOnConnection(int aRegisterVal, UBYTE aRegisterType, int aConID)

Threadsafe Syntax

int skts_pplTCAPRegister( int aRegisterVal, UBYTE aRegisterType, int aConID );

int skts_pplTCAPUnRegister( int aRegisterVal, UBYTE aRegisterType, int aConID );

Parameters

The function parameters are shown in the table below.

Argument | Description
--- | ---
aRegisterVal | OPC or Sub-System Number
aRegisterType | Registration type. Use the following constants to specify either OPC or SSN: SK_TCAP_REG_OPC (0x00) - OPC Registration SK_TCAP_REG_SSN (0x01) - SSN Registration SK_TCAP_REG_STACK_SSN 0x02 - Registers a combination of stack and subsystem number.
aConID | aConID is a connection identifier specified at connection creation time and used to indicate which LLC an application wishes to communicate with.

See Transaction Capability Application Part.
A number that addresses a node in a SS7 network.