You are here: CSP Developer’s Guide: Common Channel Signaling > 2 Introduction to SS7 > SS7 CIC Group Querying

SS7 CIC Group Querying

Overview

This host initiated feature enables the customer to determine what CIC groups are configured in order to perform detailed queries, for each CIC group, without any prior knowledge of the existing configuration. The feature supports the SS7 CIC Query (0x0067) message in order to display CIC group information:

SS7 CIC Query (0x0067) Message

This host initiated API message is used to query CIC groups for a stack as follows:

• SS7 Stack (0x08) AIB with SS7 Stack ID. Refer to the CSP API Reference for the format.

See Circuit Identification Codes.
See Signaling System Number Seven.
See Address Information Block.