0x0115 Call Agent Mode

Enables Call Agent Mode which allows bearer-free calls.

Used in:
VoIP Protocol Configure message

Byte | Description
0, 1 | Tag 0x0115
2, 3 | Length 0x0001
4 | Value[0] Call Agent Mode: 0x00 - Disables Call Agent Mode 0x01 - Enables Call Agent Mode

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).