You are here: CSP Hardware Installation and Maintenance > 2 CSP 2090/CSP 2110 Chassis Reference > Physical Specifications

Physical Specifications

CSP 2090 Specifications

The table below lists the physical specifications for the CSP 2090.

Characteristic | Specifications
--- | ---
Physical Dimensions | 39.9 cm (15.7") [H] x 43.8 cm (17.25") [W] x 48.6 cm (19.125") [D]
Weight | 29.5 kg (65 lb) (empty chassis with fan trays and blockout cards installed) 45.5 kg (100 lb) (loaded chassis)
Power Rating | –48 V DC, 25 A (maximum)
Input Voltage Range | –40 V DC to –60 V DC
Heat Dissipation | 2,400 BTUs/hr

CSP 2110 Specifications

The table below lists the physical specifications for the CSP 2110.

Characteristic | Specifications
--- | ---
Physical Dimensions | 48.9 cm (19.25") [H] x 43.8 cm (17.25") [W] x 48.6 cm (19.125") [D]
Weight | 34 kg (75 lb) (empty chassis with fan trays and blockout cards installed) 50 kg (110 lb) (loaded chassis)
Power Rating | –48 V DC, 25 A (maximum)
Input Voltage Range | –40 V DC to –60 V DC
Heat Dissipation | 2,476 BTUs/hr