0x05F2 Play File Queue

Use this TLV in the Play File Start message (0x011B) to add a file to the Play File Queue. The TLV supports all file IDs, and it works with both the Channel AIB and the Conference AIB.

If File A is playing and has not completed before you send File B, File B interrupts File A. This TLV causes File B to wait in queue so that File A can finish.

When queing files, do not use this TLV in the first playfile start message sent. Use this TLV in all other playfile start messages that are to be queued.

Byte | Description
0, 1 | Tag:0x05F2 - Play File Queue
2, 3 | Length: 0x0001
4, 5 | Value[0] 0x00 - Queue 0x01 - Override

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Address Information Block.