0x2710 Universal Protocol Data, Single

Use this TLV to specify the universal protocol data.

Used in:
PPL Table Download message

Byte | Description
0, 1 | Tag 0x2710
2 | Value[0] Data Format (See Note 1)
3 | Value[1] Offset (See Note 3)
4-7 | Value[2-5] Reserved
: | Value[:] Universal Protocol Data (See Note 2)
: | Value[:] Mask (See Note 2)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.