0x0602 Resource Type

Use this TLV to identify the resource type in the following messages:

Resource Create (0x0124)

Resource Modify (0x0125)

Resource Delete (0x0126)

Resource Connect (0x0127)

Byte | Description
0, 1 | Tag: 0x0602 - Resource Type
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Resource Type 0x0100 - Conference 0x0105 - Send Fax 0x0106 - Receive Fax 0x0107 - Child Conference 0x0108 - Echo Cancel 0x0109 - Positive Voice Detection/ Answering Machine Detection (PVD/AMD) 0x010A - Send SMS 0x010B - Receive SMS 0x010C - Send FSK 0x010D - Receive FSK

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Frequency Shift Keying