You are here: CSP Developer’s Guide: Overview > 9 Configuring the DSP-ONE Card > Hardware

Hardware

The DSP-ONE card has daughter modules that are not field-replaceable. The eight DSPs on each module are grouped logically into two "Virtual SIMMs."

A DSP-ONE card with two daughter modules, each of which has two virtual SIMMs, has a total of 16 DSP chips.

The DSP-ONE card can be populated with any of the following combinations of modules:

• One General Purpose Module (contains two logical General Purpose SIMMs)

• Two General Purpose Modules

• One VRA Module (contains one logical General Purpose SIMM and one logical VRA SIMM)

• Two VRA Modules

• One General Purpose Module and one VRA Module

Figure 9-1 SIMMs and Modules on the DSP-ONE Card

Digital Signal Processor