You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > A Appendix - TCAP Codes > ITU TCAP Codes

ITU TCAP Codes

Purpose

Refer to the following tables for the CCITT TCAP codes.

Table A-7 ITU TCAP User Abort Reason

Name | Value | Description
--- | --- | ---
TCPUABT_AC_NOT_SUP | 0x01 | Application context not supported.
TCPUABT_USER_DEFINED | 0x02 | Reason user defined.
TCPUABT_DLG_REFUSED | 0x03 | Dialogue refused.

Table A-8 TU TCAP P-Abort Reason

Name | Value | Description
--- | --- | ---
TCPPABT_ABNORMAL_DLG | 126 | Abnormal dialogue.
TCPPABT_NO_COMMON_DLG | 127 | No common dialog.
TCPABT_REASON_UNREC_MSG_TYPE | 0x00 | Unrecognized message type.
TCPABT_REASON_UNREC_TRANS_ID | 0x01 | Unrecognized transaction Id.
TCPABT_REASON_BADLY_STRUCT_TRANS_PORT | 0x02 | Badly structured transaction portion.
TCPABT_REASON_INCORRECT_TRANS_PORT | 0x03 | Incorrect transaction portion.
TCPABT_REASON_RES_UNAVAIL | 0x04 | Resource unavailable.

I

Table A-9 ITU TCAP Reject Problem Types

Name | Value | Description
--- | --- | ---
TCPPROB_GENERAL | 0x00 | General problem.
TCPPROB_INVOKE | 0x01 | Invoke problem.
TCPPROB_RETURN_RES | 0x02 | Return Result problem.
TCPPROB_RETURN_ERR | 0x03 | Return Error problem

Table A-10 ITU TCAP Reject Problem Codes

Name | Value | Description
--- | --- | ---
TCPPROB_SPEC_GEN_UNREC_COMP | 0x00 | General problem unrecognized component.
TCPPROB_SPEC_GEN_MISTYPED_COMP | 0x01 | General problem mistyped component.
TCPPROB_SPEC_GEN_BADLY_STRUCT_COMP | 0x02 | General problem badly structured component.
TCPPROB_SPEC_INV_DUPLICATE_INV_ID | 0x00 | Invoke problem duplicate invoke id.
TCPPROB_SPEC_INV_UNREC_OP_CODE | 0x01 | Invoke problem-unrecognized operation code.
TCPPROB_SPEC_INV_MISTYPED_PARAM | 0x02 | Invoke problem mistyped parameter.
TCPPROB_SPEC_INV_RESOURCE_LIMIT | 0x03 | Invoke problem resource limitation.
TCPPROB_SPEC_INV_INITIATE_RELEASE | 0x04 | Invoke problem initiate release.
TCPPROB_SPEC_INV_UNREC_LINKED_ID | 0x05 | Invoke problem-unrecognized linkedid.
TCPPROB_SPEC_INV_UNEXPECTED_LINK_RESP | 0x06 | Invoke problem unexpected linked response.
TCPPROB_SPEC_INV_UNEXPECTED_LINKED_OP | 0x07 | Invoke problem unexpected linked operation.
TCPPROB_SPEC_RES_UNREC_INVOKE_ID | 0x00 | Result problem unrecognized invoke id.
TCPPROB_SPEC_RES_UNEXPECTED_RET_RES | 0x01 | Result problem unexpected return result.
TCPPROB_SPEC_RES_MISTYPED_PARAM | 0x02 | Result problem mistyped parameter.
TCPPROB_SPEC_ERR_UNREC_INVOKE_ID | 0x00 | Error problem unrecognized invoke id.
TCPPROB_SPEC_ERR_UNEXPECTED_RET_ERROR | 0x01 | Error problem unexpected return error.
TCPPROB_SPEC_ERR_UNREC_ERROR | 0x02 | Error problem unrecognized error.
TCPPROB_SPEC_ERR_UNEXPECTED_ERROR | 0x03 | Error problem unexpected error.
TCPPROB_SPEC_ERR_MISTYPED_PARAM | 0x04 | Error problem mistyped parameter.

Comité Consultatif Internationale de Telephonique et Telegraphique (now ITU)
See Transaction Capability Application Part.
International Telecommunications Union (UN)
Connection between nodes, physical connectivity