# SwitchConnections

Specifies whether or not to nail up default connections.

#### Syntax

SwitchConnections = setting

#### Access

Read/Write

#### Type

String

#### Default

Auto

#### Allowed values

Yes | No | Auto

#### Example

SwitchConnections = Yes

#### Details

Valid entries include the following values:

Setting | Description
--- | ---
Yes | Nails up connections independent of the Clocking.HBus.ClockMode setting.
No | Does not nail up connections.
Auto | Nails up connections automatically if Clocking.HBus.ClockMode = STANDALONE.

When running the Point-to-Point Switching service, set SwitchConnections = No. Use the ppx.cfg file to define default connections. For more information, refer to the Point-to-Point Switching Service Developer's Reference Manual.

#### See also

SwitchConnectMode