# Location.PCI.Slot

Defines the logical slot location of the board on the PCI bus.

#### Syntax

Location.PCI.Slot = slotnum

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

0 - 255

#### Example

Location.PCI.Slot = 1

#### Details

Every PCI slot in the system is identified by a unique PCI bus and slot number. A PCI board is identified in the system configuration file by specifying its bus and slot number.

This statement along with Location.PCI.Bus assigns the board number to the physical board.

Use pciscan to determine the PCI bus and slot assigned for all NMS PCI boards in the system. For more information, refer to the NMS OAM System User's Manual.