# NCCEVN_HOLD_REJECTED

Request to put a call on hold was rejected.

#### State transition

None.

#### Associated function

nccHoldCall

#### Fields

Field | Description
callhd | Call handle.

#### Details

NCCEVN_HOLD_REJECTED indicates that the protocol rejected a request to put a call on hold. The call remains active.

Call hold/retrieve is not supported by all protocols. NCC_CAP_HOLD_CALL in the capabilitymask returned by nccQueryCapability indicates if the current protocol supports call hold or not.