# Incoming call events

Event | Informational/ Transitional | Solicited/ Unsolicited | Indicates that...
--- | --- | --- | ---
NCCEVN_ACCEPTING_CALL | Transitional | Solicited | The application accepted the call referenced by the call handle.
NCCEVN_ANSWERING_CALL | Transitional | Solicited | The application answered the call referenced by the call handle.
NCCEVN_CALL_CONNECTED | Transitional | Unsolicited | Both parties are connected.
NCCEVN_INCOMING_CALL | Transitional | Unsolicited | All information related to an incoming call was collected, and is now presented to the application.
NCCEVN_RECEIVED_DIGIT | Transitional | Unsolicited | Digits are being received in an overlapped fashion for an incoming call.
NCCEVN_REJECTING_CALL | Transitional | Solicited/ Unsolicited | A call is being rejected.
NCCEVN_SEIZURE_DETECTED | Transitional | Unsolicited | The network seized the line.