# IPC.AddRoute[x].Interface

Specifies the Ethernet interface (1 or 2) associated with IPv4
connections.

#### Syntax

IPC.AddRoute[x].Interface = E thernet_number

x = index of the route entry

#### Access

Read/Write

#### Type

Integer

#### Default

2

#### Allowed values

1 | 2

#### Example

IPC.AddRoute[1].Interface = 1

#### Details

Note: This keyword cannot be used in conjunction with the IPC.AddRoute[x].GatewayAddress keyword.

For more information, refer to Configuring IPv4 Ethernet connections.

#### See also

IPC.AddRoute[x].DestinationAddress, IPC.AddRoute[x].Mask