# IPv6.Link[x].NDRetranTimer

Specifies the neighbor discovery retransmission timer (in milliseconds) for the specified Ethernet interface.

#### Syntax

IPv6.Link[x].NDRetranTimer = ndretran

x = index of the link entry

#### Access

Read/Write

#### Type

Integer

#### Default

1000

#### Allowed values

100 - 60000

#### Example

IPv6.Link[1].NDRetranTimer = 2000

#### Details

This keyword configures how often the IPv6
stack retransmits neighbor solicitations when corresponding neighbor advertisements are not received. For information about neighbor discovery, refer to RFC 2461 - Neighbor Discovery for IP Version 6. For information about using board keywords to configure IPv6 Ethernet interfaces, refer to Configuring IPv6 Ethernet connections.

#### See also

IPv6.Link[x].NDAttempts, IPv6.Link[x].NDReachabilityTimer