# cnfjoin example

The following example sets up one conferencing resource. Up to 32 members can dial into the T1 link and join the conference. This example assumes you are using a CG6060 board connected to one T1 interface.

Step | Action
1 | Configure the system using c6060cnf_ivr_nonspan.cfg and cnf_c6060cnf_ivr_nonspan.cfg.
3 | Start cnfjoin by entering the following command at the prompt: cnfjoin –n 32