# oamBoardPlugins

Starts the OAM Board Plug-in table containing keywords, values, and qualifiers for each board plug-in.

#### Syntax

Object

#### Access

Not accessible.

#### OID

p.2

#### Details

The objects in the OAM Board Plug-in table are:

Object | Description
--- | ---
boardPluginTable | Top of the table.
boardPluginEntry | Begins a row of the OAM Board Plug-in table.
boardPluginIndex | Plug-in index. This value is equivalent to the index number of the BoardPlugins[x] keyword listing the board plug-in in the Supervisor managed object.
boardPluginKwIndex | Unique index (within this table) identifying the keyword.
bpikeywordName | Keyword name, formatted as described in OAM Database MIB tables and keywords.
bpikwValue | Value of the keyword.
bpikwType | Type of the keyword: integer or string.
bpikwMode | 1 indicates keyword value is read/write. 0 indicates keyword value is read-only.
bpikwAllowedRange | Range of allowable values for the keyword, formatted as described in OAM Database MIB tables and keywords.
bpikwDescription | Short description of the keyword.