# Buffer pool errors (0x0700)

The following table lists the buffer pool errors (0x0700):

Error Name | Hex | Description | Category
--- | --- | --- | ---
POOLERR_FREE_BUFFER_ADDR | 0x0701 | Attempted to free an invalid address. | 3
POOLERR_BUFFER_DOUBLE_FREE | 0x0702 | Double buffer free. | 3
POOLERR_BUFFER_OVERRUN | 0x0703 | Buffer was overrun. | 3
POOLERR_BUFFER_ADDR_NOT_MOD | 0x0704 | Attempted to free an invalid address. | 3
POOLERR_ALLOC_SIZE_TOO_LARGE | 0x0705 | Too large an allocation. | 3
POOLERR_BUFFER_POOL_EMPTY | 0x0706 | No more buffers. | 3
POOLERR_COULD_NOT_CREATE | 0x0707 | No more memory. | 3