# MCC_SDP_ADDRESS

Represents an SDP origin address or connection address.

#### Definition

typedef struct _MCC_SDP_ADDRESS
{
const char * nettype;
const char * addrtype;
const char * address;
} MCC_SDP_ADDRESS;

#### Fields

Field | Type | Description | SDP field | Required/ optional
nettype | const char | Network type. Recognized value is MCCSDP_NETTYPE_IN (Internet address). | o or c | Required
addrtype | const char | Address type. Recognized values are: MCCSDP_ADDRTYPE_IP4 MCCSDP_ADDRTYPE_IP6 | o or c | Required
address | const char | Destination IP address. | o or c | Required