# AutoStart

Specifies whether the board automatically starts when ctdaemon is started.

#### Syntax

AutoStart = argument

#### Access

Read/Write

#### Type

String

#### Default

NO

#### Allowed values

YES | NO

#### Example

AutoStart = NO

#### Details

The Supervisor keyword AutoStartEnabled enables or disables the autostart feature. If AutoStartEnabled is set to YES, the Supervisor starts each board whose AutoStart keyword is set to YES when ctdaemon is started. If AutoStartEnabled is set to NO, no boards are started automatically, regardless of the setting of the AutoStart keyword.

For details, refer to the NMS OAM System User's Manual.

#### See also

AutoStop