# DSP.C5x[x].Image

Specifies the DSP image file for the processor.

#### Syntax

DSP.C5x[x].Image = filename

x = 0..3

#### Access

Read/Write

#### Type

File name

#### Default

None.

#### Allowed values

A valid file name.

#### Example

DSP.C5x[1].Image = ag2fax.c54

#### Details

Specifies a pre-linked DSP image file for AG boards used by developers to develop their own DSP images.

The naming convention for DSP image files is filename.c54.

Setting DSP.C5x[x].Image = NULL leaves the specified DSP(s) in an unbooted state.