# Error type FF00 (Linux only)

The following table lists FF00 type (host driver) errors:

Error code | Error name | Additional information returned | Category
-22 | AGERR_MSG_BALANCE_LOST | Channel, message. | 3
-42 | AGERR_LESS_THAN_48_BYTES | SRAM words left. | 3
-43 | AGERR_RECEIVE_MSG_COUNT | Count left. | 3
-44 | AGERR_AGMSG_DATA | Buffer count, parameter count. | 3
-100 | AGERR_NO_STREAMS_MSG_BLOCK | Channel, message. | 3