# Filter manager errors (0x0200)

The following table lists the filter manager errors (0x0200):

Error name | Hex | Description | Category
--- | --- | --- | ---
FM_ERROR_INVALID_HANDLE | 0x0202 | Invalid handle to the filter manager. | 1
FM_ERROR_OUT_OF_MEMORY | 0x0203 | No more memory in the filter manager. | 3
FM_ERROR_INVALID_PARAMETER | 0x0204 | Invalid parameter in a function call. | 1
FM_ERROR_PIN_CONNECT_FAILED | 0x0205 | Could not connect the pins. | 1
FM_ERROR_UNKNOWN_FILTER_TYPE | 0x0206 | Filter type (DSP function) unrecognized. | 4
FM_ERROR_LIMITED_OR_NO_RESOURCES_FOUND | 0x0207 | Not enough resources. | 4
FM_ERROR_RM_NUM_ENTIRES_TOO_LARGE | 0x0208 | Not enough resources. | 4
FM_ERROR_DEFRES_OUT_OF_MEMORY | 0x0209 | No more memory. | 3