# dsx1CurrentIndex

Number of the DS1 interface to which a block of variables apply.

#### Syntax

Integer

#### Access

Read-only

#### OID

p.7.1.1.n, where n = the index number of the DS1 interface.

#### Details

The following block of variables apply to Hot Swap:

If a board is... | Then the...
--- | ---
Extracted | Index is removed.
Inserted | Next available index number is used.
Replaced | Next available index number is used.

This variable is the same as dsx1LineIndex in the Trunk Configuration table.