# Executive errors (0x0500)

The following table lists the executive errors (0x0500):

Error name | Hex | Description | Category
--- | --- | --- | ---
EXEC_ERROR_OUT_OF_MEMORY | 0x0502 | No more memory. | 3
EXEC_ERROR_INVALID_PARAM | 0x0503 | Invalid parameter in a function call. | 1
EXEC_BOARD_ALREADY_INIT | 0x0552 | Board was reconfigured without a reset. | 3
EXEC_INCOMPATIBLE_CORE_VERSION | 0x0555 | Flash needs to be updated with burnall. | 4
EXEC_WATCHDOG_FIRED | 0x0556 | Board usage has reached 100 percent or low priority tasks are blocked. | 4